{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["工程量明细"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量明细","index":0,"n_rows":15,"n_cols":10,"rows_kept":15,"merged":[[0,0,0,9],[1,3,1,5],[2,0,13,0],[2,1,9,1],[2,3,2,5],[2,6,9,6],[3,3,3,5],[4,3,4,5],[5,3,5,5],[6,3,6,5],[7,3,7,5],[8,3,8,5],[9,3,9,5],[10,3,10,5],[11,1,12,1],[11,3,11,5],[12,3,12,5],[13,3,13,5],[14,0,14,6],[15,0,15,6],[16,6,16,9]],"flags":["formulas_cached_only"]}
["潞城市 潞安·颐龙湾住宅小区节能专项检测明细表"]
["检验类别","分项工程","材料名称","复验项目",null,null,"复验数量要求","检验批","单价","合价"]
["节能材料进场复检","墙体节能  工程","XPS","   导热系数、表观密度、压缩强度",null,null,"同厂家、同品种的产品，按照扣除门窗洞口后的保温墙面面积所使用的材料用量，在5000㎡以内时应复验一次，面积每增加5000㎡应增加一次（增加的面积不足规定数量也应增加一次）。\n地面、屋面保温：\n同厂家同品种产品，地面面积在1000㎡以内时应复验一次；面积每增加1000㎡应增加复验一次。",7]
[null,null,"岩棉板","  导热系数、表观密度、压缩强度     ",{"$nulls":3},7]
[null,null,"燃烧性能","B1级燃烧性能 ",{"$nulls":3},9]
[null,null,"燃烧性能","A级燃烧性能 ",{"$nulls":3},7]
[null,null,"粘结砂浆","拉伸粘结强度",{"$nulls":3},3]
[null,null,"抹面砂浆","拉伸粘接强度、压折比",{"$nulls":3},3]
[null,null,"耐碱网布"," 单位面积质量、耐碱断裂强力、耐碱断裂强力保留率      ",{"$nulls":3},3]
[null,null,"保温钉","抗拉承载力",{"$nulls":3},3]
[null,"楼梯间","保温砂浆","干密度、抗压强度",{"$nulls":3},2]
[null,"供暖节能 工程","管材","纵向回缩率、静液压试验",null,null,"/",2]
[null,null,"EPS","   导热系数、表观密度、压缩强度       ",null,null,"/",2]
[null,"门窗工程","外窗","气密性、水密性、抗风压、保温性能、中空露点",null,null,"窗户200樘做一组。现场检测按建筑面积为30000平米做一组。",3]
["总  计"]